|  |  |
| --- | --- |
| Test 130, MSD40NBT current test. |  |
| Linux | 20121203 |
| Fluke 87 Meter |  |
| MSD40NBT Rev 11 |  |
| Firmware | ABGN, No CCX, Full IOCTL |
| D Chapman & B Wagner | 14-Jan-13 |
| **Mode** | **Current, ma** |
| Wi-Fi on  & connected, BT not initialized. | 11 |
| Wi-Fi on & connected, BT on & firmware loaded. | 14 |
| Wi-Fi on & connected, BT in sleep. | 4 |
| Wi-Fi on & connected, BT transmitting. | 29 |
| Wi-Fi on & connected, BT connected to BT device. | 29 |
| Wi-Fi on and connected, BT held in reset. | 4 |